**SECTION 10 14 16**

**PLAQUE**

**PART 1 GENERAL**

1. RELATED DOCUMENTS
   1. Drawings and general provisions of the Contract, including General and Supplementary Conditions and Division 1 specification section, apply to work of this section.
2. SECTION INCLUDES
   1. Cast aluminum dedication plaque at location and design as shown on architectural drawings.
3. REFERENCE
   1. School Board Policy 7.041 - Dedicatory plaque in new schools: Place the names of the School Board Members, the Board Chairman, and the Superintendent who are in office at the time of awarding the construction contract for a new facility or major addition.
4. SUBMITTAL
   1. Submit under provisions of Section 01 33 00.
   2. Provide shop drawing of plaque size, border type, background finish, letter styles, and sizes, and mounting method.
      1. Verify names, titles and exact wording required for plaque prior to fabrication.
   3. Provide rubbing of actual pattern for architect’s approval prior to casting.
5. QUALIFICATIONS
   1. Manufacturer: Company specializing in manufacturing the product specified in this section with minimum 5-years documented experience.

**PART 2 PRODUCT**

1. ALUMINUM TABLET
   1. Aluminum Alloy F-214, size 18" x 24" beveled edges, square corners.
2. ANCHORS
   1. Provide matching anchors suitable for secure attached to intended wall.

**PART 3 EXECUTION**

1. Casting shall be free of pits, gas holes and all letters shall be sharp, and hand tooled.
2. Clean, etch, and treat plaque with Aldine.
3. Spray two coats of clear acrylic lacquer on completed plaque.

END OF SECTION